PRODUCT

|  |  | PARDAZESH CONTROL SADRA
|  | PRODUCT

|  | PCS USB TO RS232 | PCS USB TO RS485 | PCS USB TO IrDA |
PCS USB TO MPI/DP | PCS USB TO TTY | PCS USB TO LOGO ! |
PCS USB TO PPI | PCS RS232 TO PPI | PCS RS232 TO TTY |
| PCS RS232 TO LOGO ! |  |

USB TO RS232 |  |

Congratulations on your purchase of the USB-Serial adapter.

This device provides a simple and easy way to connect Universal Serial Bus (USB) and Serial port interface.

With the advantage of USB port, users have the capability to utilize the peripheral with serial port interface in an easy to use environment such as plug and play & hot swap function.

This adapter is designed for ideal connections to Cellular Phone, Digital Camera, Modems or ISDN terminal adapter with over 1Mbps data transfer rate.

Back to top |  |
USB TO RS485 (new) |  |

The USB TO RS485 is a small USB to RS485 converter designed for industrial and commercial applications where RS485 is used because of its reliable long range of communications, high speed, multi-drop and differential transmission mode via simple twisted-pair cable.

Back to top |  |
USB TO MPI/DP (new) |  |
The PCS USB TO MPI cable connects the Programming Device or the PC over a USB 2.0 interface with the MPI or DP/FMS-Interface of a S7-300/400. The communication with this cable uses a virtual COM-port. |  |
Back to top |  |
USB TO TTY (new) |  |

The PCS USB TO TTY is a active cable for connecting a Siemens S5-PLC Port to the PC USB-Port.

The cable is be connected to the 15pin TTY port of the PLC or CP and is connected to the PC USB-Port.

The software-driver are run able for Windows 98, Me and WIN2000 and Windows XP. The communication with this cable uses a virtual COM-port. Only original 32bit-programms can work with this driver.

Back to top |  |
RS232 TO LOGO ! |  |
RS232 TO LOGO is a LOGO!-to–PC link. this adaptor connect the LOGO! to a serial port of PC . |  |
Back to top
USB TO LOGO ! (new)
USB TO LOGO is a LOGO!-to–PC link. this adaptor connect the LOGO! to a USB port of PC .
Back to top |  |
USB TO PPI (new) |  |
The USB TO PPI cable allows you to connect the USB port of a personal computer to the port of an S7-200 CPU. The USB TO PPI cable can also be used to connect the communication port of an S7-200 CPU to other USB compatible devices. |  |
Back to top |  |
RS232 TO PPI |  |

The USB TO RS232 cable allows you to connect the

RS-232 port of a personal computer to the RS-485 port of an S7-200 CPU.

The RS232 TO PPI cable can also be used to connect the communication port of an S7-200 CPU to other RS-232 compatible devices.

Back to top |  |
RS232 TO TTY |  |
The PCS RS232 TO TTY is a active cable for connecting a Siemens S5-PLC Port to the PC RS232-Port. The cable is be connected to the 15pin TTY port of the PLC or CP and is connected to the PC RS232-Port. |  |
Back to top |  |
USB TO IrDA As soon as Back to top |  |